Car Tire Changer KT-T810:  Including Bead Seater

	Max Wheel Diameter :
	41"/1040mm

	Max Wheel Width :
	15"/380mm

	Outside Clamp:
	12"-22"

	Inside Clamp :
	14"-24"

	Power Supply:
	120V 1PH

	Motor Power:
	2.0HP/1.5KW

	Rotation Speed :
	6.8r/min

	Air Pressure :
	0.8-1.0Mpa(116-145psi)

	Net weight :
	186KG



--Alloy steel jaw, interface carburization treatment of 0.8-1.1mm deepness, whole quenching process, making the jaw inside more tenacity and outside more hard, and take the jaw cover for protect rim.
--The mounting head is made by stainless, solution treatment and interface polishing, the shape conforms to the engineering principle,and take with plastic cover for protect rim.     
-- Inflation gauge with pedal control.     
--With high quality spade cover, effective prevent damage rim.     
--Pull type pedal control system, convenience for changing and maintenance.     
--Top level motor and pure copper winding, fast heat dissipation,low defect rate and longer using life.     
--With high quality filter, reliable drop oil, effective filter pressure air,and make more longer using life for pneumatic system.     
--For North America region used 120V/1ph/2.0HP motor,more strong power and high efficiency working.     
--Closed body for protect inside parts well.      

